Product ID:VARATHANE CLEAR LIQUID PLASTIC #90 GLOSS

MSDS Date:01/01/1985

FSC:8010

NIIN:00N000575

MSDS Number: BCFTP

=== Responsible Party ===

Company Name:FLECTO COMPANY \*

Address:1000 45TH STREET \*

City:OAKLAND \*

State:CA

ZIP:94608

Country:US

Info Phone Num:415-655-2470 \*

Emergency Phone Num:415-655-2470 \*

CAGE:GO894

=== Contractor Identification ===

Company Name:FLECTO CO INC

Address:1000 45TH ST

Box:City:OAKLAND

State:CA

ZIP:94608-3314

Country:US

Phone:800-635-3286

CAGE:58381

Company Name:FLECTO COMPANY \*

Address:1000 45TH STREET \*

Box:City:OAKLAND \*

State:CA

ZIP:94608

Country:US

Phone:415-655-2470 \*

CAGE:GO894

============= Composition/Information on Ingredients =============

Ingred Name:NAPHTHA (PETROLEUM SPIRITS OR BENZIN)

CAS:8030-30-6

RTECS #:SE7555000

OSHA PEL:100 PPM

Ingred Name:TOLUENE (SARA III)

CAS:108-88-3

RTECS #:XS5250000

Fraction by Wt: 7.2%

OSHA PEL:200 PPM/150 STEL

ACGIH TLV:50 PPM; 9293

EPA Rpt Qty:1000 LBS

DOT Rpt Qty:1000 LBS

Ingred Name:ACETONE (SARA III)

CAS:67-64-1

RTECS #:AL3150000

Fraction by Wt: 14.4%

OSHA PEL:1000PPM

ACGIH TLV:750PPM/1000STEL;9293

EPA Rpt Qty:5000 LBS

DOT Rpt Qty:5000 LBS

Ingred Name:N-BUTYL ALCOHOL (SARA III)

CAS:71-36-3

RTECS #:EO1400000

Fraction by Wt: 3.0%

OSHA PEL:100 PPM

ACGIH TLV:S, C 50 PPM; 9293

EPA Rpt Qty:5000 LBS

DOT Rpt Qty:5000 LBS

Ingred Name:ALIPHATIC & HALOGENTATED ALIPHATIC HYDROCARBONS

 (PROPELLENT)

Fraction by Wt: 39.5%

===================== Hazards Identification =====================

Effects of Overexposure:ACUTE: INH OF HIGH VAP CONC MAY CAUSE DIZZINESS

 OR NAUSEA. AVOID EYE CONTACT & PRLNGD SKIN CONTACT.

======================= First Aid Measures =======================

First Aid:EYE: FLUSH IMMED W/WATER FOR 15 MIN. SKIN: WASH W/WATER. INH:

 PROMPT REMOVAL TO FRESH AIR. INGEST: DO NOT INDUCE VOMITING - CALL

 PHYSICIAN.

===================== Fire Fighting Measures =====================

Flash Point:105F TCC

Lower Limits:1.3

Extinguishing Media:CO\*2, ALCOHOL FOAM, DRY CHEMICAL

Fire Fighting Procedures:USUAL PROCEDURES FOR PAINT

================== Accidental Release Measures ==================

Spill Release Procedures:REMOVE ALL SOURCES OF IGNITION (FLAMES, HOT

 SURFACES, SPARKS, STATIC) AVOID BREATHING VAPORS. VENTILATE AREA.

 REMOVE W/INERT ABSORBENT.

====================== Handling and Storage ======================

Other Precautions:NORMAL PAINT PRECAUTIONS. COMBUSTIBLE MIXTURE. DO NOT

 USE NEAR FIRE OR FLAME. DO NOT TAKE INTERNALLY. KEEP AWAY FROM

 CHILDREN.

============= Exposure Controls/Personal Protection =============

Ventilation:USE GOOD VENTILATION

Protective Gloves:NEOPRENE/RUBBE

Eye Protection:SAFETY GOGGLES

Supplemental Safety and Health

WT PER GAL:7.54 LBS.ADD INGRED:(NON-VOLATILE)POLYHYDRIC ALCOHOL

 ESTERIFIED W/LINOLENIC OLEIC,PALMITIC & STEARIC ACIDS & MODED

 W/TOLUENE DIISOCYANATE.MFR STATES: ZERO TDI - CMPTLY REACT

================== Physical/Chemical Properties ==================

HCC:F4

Boiling Pt:B.P. Text:315-390F

Vapor Pres:>1.

Vapor Density:0

Evaporation Rate & Reference:SLOWER THAN ETHER

Percent Volatiles by Volume:68.9

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

==================== Disposal Considerations ====================

Waste Disposal Methods:DO NOT INCINERATE IN CLOSED CONTAINERS. USE

 NORMAL PAINT DISPOSAL METHODS IN ACCORDANCE W/FED., STATE & LOCAL

 REGULATIONS.

 Disclaimer (provided with this information by the compiling agencies):

 This information is formulated for use by elements of the Department

 of Defense. The United States of America in no manner whatsoever,

 expressly or implied, warrants this information to be accurate and

 disclaims all liability for its use. Any person utilizing this

 document should seek competent professional advice to verify and

 assume responsibility for the suitability of this information to their

 particular situation.